LOWERING CRADLE ASSEM.A,X CARS DISCONNECT RACK/PIN.STRG.GEAR. Chevrolet Celebrity 1982

For 1990-2009 cars

# LOWERING CRADLE ASSEM.A,X CARS DISCONNECT RACK/PIN.STRG.GEAR

ANYTIME THE CRADLE ASSEMBLY IS LOWERED AT THE REAR FOR ACCESS TO THE DISTRI- BUTOR OR OTHER COMPONENTS, THE RACK AND PINION STEERING GEAR ASSEMBLY MUST BE DISCONNECTED FROM THE INTERMEDIATE SHAFT. FAILURE TO DO SO MAY RESULT IN DAMAGE TO THE INTERMEDIATE SHAFT.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.