WARPED LEFT FRT. DOOR INTERIOR HANDLE ESCUTCHEON (NEW PART). Chevrolet Celebrity 1987

For 1990-2009 cars

# WARPED LEFT FRT. DOOR INTERIOR HANDLE ESCUTCHEON (NEW PART)

VEHICLES-AFFECTED: 1987 CHEVROLET CELEBRITY W/POWER WINDOWS

A redesigned left front door remote handle trim escuthcheon P/N 10125701, has been released for service to address owner comments of warpage on 1987 Celebrities with power windows. The new escutcheons have two (2) retaining legs added to the upper edge to prevent warping. Therefore, some modification is required to the door trim panel. To install a new escutcheon use the following procedure.

#### Procedure:

1. Remove front door remote handle trim escutcheon.

2. Using template provided, mark area of door trim pad to be cut out. Align new escutcheon to trim pad to insure area marked for removal is correct, and using a sharp blade make cut-outs.

3. Install new escutcheon

Use the most applicable Labour Operation and time from the Canadian Labour Time Guide.

***************************************************************************** *STG DISCLAIMER*

"THE TEMPLATE DISPLAYED IN THIS SERVICE PUBLICATION IS NOT INTENDED FOR USE" (Please refer to the actual publication for an accurate "TEMPLATE" to use in this service procedure.) *****************************************************************************

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.