BRAKES BIND/SLOW PEDAL RETURN PUSH ROD & PEDAL ARM BIND. Chevrolet Celebrity 1986

For 1990-2009 cars

# BRAKES BIND/SLOW PEDAL RETURN PUSH ROD & PEDAL ARM BIND

#### VEHICLES AFFECTED ALL 1982-87 'A' CARS

Some 1987 vehicles may experience a slow or incomplete service brake pedal return as a result of slight bind between the eyelet end of the brake booster pushrod and brake pedal arm attaching hardware. This condition can be repaired by replacing the original flat washer with a new precision, hardened washer. Adequately lubricate the pushrod and washers and retorque attaching nut, P/N 11500756, to 35 Nm. After installing the new washer, recheck for slow or incomplete service brake pedal return by lightly applying the service brake several times with the engine running and observing the pedal return.

New P/N Old P/N

10087739 25501227

Use applicable labour operation number and time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.