REAR 1/4 TRIM FINISH PANEL CORRECTION FOR LOOSE PANEL. Chevrolet Celebrity 1984

For 1990-2009 cars

# REAR 1/4 TRIM FINISH PANEL CORRECTION FOR LOOSE PANEL

#### Model and Year 1984 CELEBRITY

If a loose rear quarter trim finishing panel to fasteners are encountered, the condition may be repaired by installling the fastener to the trim panel using adhesive backed body side molding foam tape (3M-06380 or equivalent) followed by the installation of cloth-backed waterproof body tape as shown in the illustration below. The cloth-backed tape is used to provide adequate retention of fastener to trim panel and prevent peel load on tape.

Labor Operation Number: T0123 Labor Time : .2 hours one or both sides

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.