125 SEAL RING INSTALLATION TOOL AND SIZING TOOL-UPDATE. Chevrolet Celebrity 1986

For 1990-2009 cars

# 125 SEAL RING INSTALLATION TOOL AND SIZING TOOL-UPDATE

#### VEHICLES AFFECTED: 1986 All with THM 125C

Use the following information to update the THM 125C automatic transaxle section of the 1986 Service Information Manuals.

Shown in Figure 1 below, the green coloured turbine shaft seal rings (105) require the use of installation tool no. J-29569-1 and sizing tool no. J-29569-2. The yellow coloured turbine shaft seal ring requires the use of installation tool no. J-29829-1 and sizing tool no. J-29829-2.

Use Figure 1 to update the corresponding figure the THM 125C automatic transaxle section of the service information manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.