HOOD PROP ROD RATTLE ELIMINATION OF NOISE. Chevrolet Celebrity 1982

For 1990-2009 cars

# HOOD PROP ROD RATTLE ELIMINATION OF NOISE

A hood prop rod rattle in a 1982 Celebrity can be eliminated by the installation of a 20" length of hose 3/8" (9mm) Inside Diameter and 9/16" (15mm) Outside Diameter, starting at the base of the rod, and secured with 3M8001 or 3M8008 (or equivalent). (See Figure 1.)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.