LOOSE RADIO SPEAKER GRILL NOISE FROM INSTRUMENT PANEL. Chevrolet Celebrity 1988

For 1990-2009 cars

# LOOSE RADIO SPEAKER GRILL NOISE FROM INSTRUMENT PANEL

#### Model and Year: 1987-88 CELEBRITY

Comments may be received concerning loose radio speaker grilles rattling and popping up from I/P. To repair, use the following procedure:

1. Remove speaker grille from I/P.

2. Cover rear edge of grille and flange with a shop cloth to prevent damage to painted surfaces (See Illustration).

3. Using pliers, bend rear edge of grille flange slightly (approximately 3.Omm) to increase contact retention to I/P. See Illustration - Section A-A.

#### NOTICE: CARE MUST BE USED SO AS NOT TO MAR PAINTED SURFACE OF GRILLE AND/OR IP AREA.

Labor Operation Number: R0910 and R0911

Labor Time: .3 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.