INSTRUMENT CLUSTER (PRNDL) INDICATOR REPLACEMENT. Chevrolet Celebrity 1985

For 1990-2009 cars

# INSTRUMENT CLUSTER (PRNDL) INDICATOR REPLACEMENT

#### VEHICLES AFFECTED: 1985 Chevrolet Celebrity

The following procedure was inadvertently omitted from Section 8C of the 1985 Celebrity Shop Manual (ST 365-85).

1. Disconnect battery ground cable.

2. Remove steering column lower trim cover.

3. Remove I.P. pad attaching screws (8) and remove pad.

4. Remove headlight switch knob and holddown and remove I.P. cover at left side (lower) for access to cluster screws.

5. Remove cluster lens cover.

6. Remove cluster from I.P.

7. Remove two indicator to cluster attaching screws.

8. Disassemble indicator.

9. Reverse procedure to install.

10. Adjust indicator needle as required.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.