REAR STORAGE BOX LID RATTLE. Chevrolet Celebrity 1987

For 1990-2009 cars

# REAR STORAGE BOX LID RATTLE

#### VEHICLES AFFECTED: 1987 OLDSMOBILE "A " CAR WITH BA6 OPTION -----------------

A few 1987 Oldsmobile "A" styles with option BA6 (Box Assembly stowage, rear seat to, back window foundation) may exhibit a rattle condition from the stowage box lid.

To repair this condition spacer/bumpers should be added to the box at locations indicated on the Illustration.

The spacer/bumpers can be cut from 3M single coated vinyl foam #4508 or equivalent. Spacer/bumpers should be approximately 3/8 inch square.

3M #6375 is 1/8 inch th0062ick, 3M #6373 is 1/4 inch thick and may be used if required.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.