RACK/PINION POWER STEERING VALVE RING SERVICE. Chevrolet Celebrity 1984

For 1990-2009 cars

# RACK/PINION POWER STEERING VALVE RING SERVICE

#### Model and Year 1981-84 CHEVETTE, 1982-84 CAVALIER, CELEBRITY, CITATION AND 1984 CORVETTE

This bulletin supersedes the information given in Bulletin 81-T-47.

Orange color valve rings have been phased into 1984 production, replacing the green rings. The present green ring service kit, P/N 7840573, may be used to replace orange rings as they are interchangeable.

The design intent is that valve rings will remain stationary in the bore of a power rack and pinion assembly. If hard steering, lack of assist when started cold, etc., is encountered with normal pump pressure, inspect the rack and pinion housing valve bore (see illustration).

Ring contact marks in the valve bore is normal. If ring groove wear exists, replacement of the housing is necessary to assure that replacement rings will not eventually wear further into the housing and result in a recurrence of a lack of power assist symptom.

If only one (1) or two (2) of the four (4) ring contact marks in the housing have resulted in ring groove wear, the corresponding ring land of the valve is most likely causing excessive ring drag. Replacement of the valve as well as the housing would then be required.

In mid-1984, the rack and pinion housing valve bore will have a textured finish to further insure valve ring retention to the bore. The textured area in the bore will be the circular band sealing ring surface corresponding to the four (4) rings in the valve body.

#### NOTICE: 1980-81 Citations power rack and pinion assemblies are to be serviced as instructed in Dealer Technical Bulletin 81-T-83.

SERVICE PRECAUTION ON REMOVAL OF VALVE AND PINION ASSEMBLY

The valve and pinion assembly must be pressed out of the housing per Chassis Service Manual procedure. Excessive force or hammer use will likely damage the valve or valve pinion pin. After valve removal, inspect the valve pinion pin for being loose, bent, or protruding beyond the valve machined surface (see illustration). If any of these conditions exist, valve body replacement is required.

A lack of power assist symptom may also be caused by leakage past the rack piston ring in the housing tube bore. Inspect the rack piston ring for damage or distortion. The piston ring to ring land side clearance should not exceed .008". Also inspect the housing tube bore for any nicks, scoring or other imperfection in the rack piston travel area.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.