GLOVE BOX LOCK NOT ENGAGING WHEN KEY IS TURNED. Chevrolet Celebrity 1987

For 1990-2009 cars

# GLOVE BOX LOCK NOT ENGAGING WHEN KEY IS TURNED

#### Model and Year: 1984-88 CELEBRITY

Comments may be received that the glove box lock does not lock when the key cylinder is turned to the lock position. To address this condition:

1. Remove lock assembly from glove box door.

2. Remove pawl from back of lock cylinder by removing retainer clip.

3. Bend pawl down approximately 3.0mm as Illustrated.

4. Reinstall pawl and lock cylinder and check for secure lock action by turning lock cylinder with key, and then pulling on door finger area.

Labor Operation Number: C2100

Labor Time: .3 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.