TIRE CHAIN USAGE ON CELEBRITY'S WITH DIESEL ENGINE. Chevrolet Celebrity 1982

For 1990-2009 cars

# TIRE CHAIN USAGE ON CELEBRITY'S WITH DIESEL ENGINE

Tire chains, SAE class "S" type, can be used on P195/75R14 tires standard on 1982 Celebrity models equipped with a diesel engine. Because clearance to inner fender panel is limited, chains should be checked periodically for tightness, and maximum speed vehicle should be driven while chains are installed is 30 MPH.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.