T.V. CABLE ADJUSTMENT PROC. TO INSURE WOT DOWNSHIFT. Chevrolet Celebrity 1982

For 1990-2009 cars

# T.V. CABLE ADJUSTMENT PROC. TO INSURE WOT DOWNSHIFT

#### VEHICLES AFFECTED; ALL AUTOMATIC TRANSMISSIONS USED WITH GAS OR DIESEL ENGINES EXCEPT THM 400 SINCE 1981.. THE FOLLOWING PROCEDURE SHOULD BE USED WHENEVER THE T.V. CABLE HAS TO BE READJUSTED. SHIFT POINTS AND THE DURABILITY OF THE TRANS. CAN BE AFFECTED BY THIS ADJUSTMENT... 1. ENGINE MUST BE OFF. 2. RESET CABVLE TO READJUST POSITION: - DEPRESS AND HOLD METAL READJUST TAB. - MOVE SLIDER BACK THROUGH FITTING AWAY FROM THROTTLE LEVER UNTIL SLIDER STOPS AGAINST FITTING. - RELEASE READJUST TAB. 3. ADJUST CABLE: - ROTATE THROTTLE LEVER TO WIDE-OPEN-THROTTLE. - SLIDER MUST RATCHET (CLICK). IF NOT, REFER TO REPAIR PROCEDURE. 4. REVIEW SYSTEM FOR PROPER OPERATION BYM DRIVING VEHICLE AND CHECKING FOR AVAILABILITY OF WIDE-OPEN-THROTTLE DOWNSHIFTS (INTO PASSING GEAR). (ILLUSTRATION AVAILABLE ON BULLETIN)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.