ECM TERMINAL VOLTAGE CORRECTION TO CHASSIS MANUAL. Chevrolet Celebrity 1987

For 1990-2009 cars

# ECM TERMINAL VOLTAGE CORRECTION TO CHASSIS MANUAL

Page 6E2-A-6 of the 1987 Celebrity Service Manual contains an error. The voltage reading at Pin B9 (Ignition Ref. Hi) should be about:

Key "On" = 4.5V Eng. Run = 3.0V

Please make note of this on the page referenced above.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.