WINDSHIELD WASHER SLOW INSTALL CHECK VALVE. Chevrolet Celebrity 1984

For 1990-2009 cars

# WINDSHIELD WASHER SLOW INSTALL CHECK VALVE

#### Model and Year 1984 CELEBRITY AND MONTE CARLO

The washer system response time on permanent magnet type wipers used on 1984 Celebritys and Monte Carlos may be reduced by installing a check valve, P/N 25504746, in the fluid pick-up hose. To install the check valve, cut the pick-up hose off 2" from the washer pump and insert the valve. Be sure to ob- serve the direction of flow through the valve. The valve will prevent fluid drain back and reduce the washer response time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.