VINYL WINDSHIELD REVEAL MOLD'G REMOVAL AND INSTALLATION. Chevrolet Chevette 1981

For 1990-2009 cars

# VINYL WINDSHIELD REVEAL MOLD'G REMOVAL AND INSTALLATION

WINDSHIELD REVEAL MOLDING THE WINDSHIELD REVEAL MOLDING IS MADE OF VINYL AND IS RETAINED TO THE BODY BY URETHANE ADHESIVE. REMOVAL TO REMOVE VINYL WINDSHIELD REVEAL MOLDING, SLIDE ESCUTCHEON, LOCATED AT TOP CENTERLINE OF MOLDING, TO ONE SIDE, EXPOSING BUTT JOINT OF MOLDING. USE CARE AND PRY ONE EDGE OF MOLDING OUT OF URETHANE. ONCE MOLDING IS REMOVED ABOUT 75 MM(3"), GRASP MOLDING BY HAND AND SLOWLY PULL MOLDING AWAY FROM BODY UNTIL ENTIRE MODLING HAS BEEN REMOVED. * ADDITIONAL TEXT IN BULLETIN *

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.