REAR COMPARTMENT LID WEATHERSTRIP SEAL OOZE-OUT. Chevrolet Chevette 1981

For 1990-2009 cars

# REAR COMPARTMENT LID WEATHERSTRIP SEAL OOZE-OUT

TO CORRECT A DECK LID WEATHERSTRIP SEALER OOZE OUT CONDITION ON ANY OF THE ABOVE VEHICLES, NEW SEALERLESS WEATHERSTRIPS HAVE BEEN RELEASED FOR SERVICE ONLY.

PART NUMBER FOR SEALERLESS WEATHERSTRIPS:

CAVALIER 27-69 20470877 CAMARO 87 20471808 CAVALIER 77 20470878 CHEVETTE 08-68 20470876 CITATION 08-68 20465850

SHOULD IT BECOME NECESSARY TO REPLACE A REAR COMPARTMENT OR HATCH LID WEATHERSTRIP FOR ANY REASON, REFER TO THE FOLLOWING PROCEDURE:

REAR COMPARTMENT LID WEATHERSTRIP SEALER OOZE OUT CORRECTION

1. REMOVE OLD WEATHERSTRIP AND CLEAN ALL SEALER FROM FLANGE AROUND ENTIRE OPENING.

2. BRUSH 3M 8011 BLACK WEATHERSTRIP ADHESIVE OR EQUIVALENT ON BOTH SIDES OF THE FLANGE COMPLETELY AROUND THE OPENING.

3. APPLY A BEAD OF 3M 8011 OR EQUIVALENT INTO THE NEW WEATHERSTRIP CARRIER. ALLOW TO DRY UNTIL ADHESIVE BECOMES TACKY(APPROXIMATELY 5 MINUTES).

4. INSTALL NEW WEATHERSTRIP TO FLANGE AND ALLOW A MINIMUM OF 3 HOURS BEFORE CLOSING LID.

5. CLOSE LID AND WATER TEST REAR COMPARTMENT (MINIMUM 4 MINUTES).

6. IF WATERLEAKS OCCUR:

A. BE SURE WEATHERSTRIP IS FULLY SEATED ON FLANGE. B. APPLY ADDITIONAL 8011 OR EQUIVALENT UNDER WEATHERSTRIP OUTER LIP. C. REPEAT STEP 5.

LABOR OPERATION NUMBER T0078 LABOR TIME .7 HOURS

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.