'CS' EMBLEM MISSING INSTALL ON DECK LID. Chevrolet Chevette 1984

For 1990-2009 cars

# 'CS' EMBLEM MISSING INSTALL ON DECK LID

#### Model and Year 1984 CHEVETTE "CS" SERIES VEHICLES

Some 1984 Chevette "CS" series may be missing the deck lid "CS" emblems. Chevette "CS" series vehicles can be identified by the appearance of the letter B at the fifth position of the vehicle serial number.

The "CS" emblem, P/N 14044267, can be ordered from WDDGM.

SERVICE PROCEDURE

1. Clean area of body surface where emblem is to be applied with a suitable solvent (oil free-naptha or alcohol). Use clean cloth only.

2. Dry surface with clean cloth.

3. Body and emblem temperature at time of emblem application should be 70 DEG F to 90 DEG F.

Adhesive surface must not be touched or brought in contact with any surface or foreign matter.

4. Apply emblem to LH side of rear deck lid per attached sketch and press firmly in place.

Use applicable labor operation.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.