POWER STEERING SHUDDER REPLACE POWER STEERING HOSE. Chevrolet Citation 1981

For 1990-2009 cars

# POWER STEERING SHUDDER REPLACE POWER STEERING HOSE

#### CONDITION:

A POWER STEERING SHUDDER ON 1981 OMEGA'S MAY BE ENCOUNTERED WHEN THE STEERING GEAR IS NEAR THE END OF ITS TRAVEL AT EITHER THE RIGHT OR LEFT STOP; SUCH AS STATIONARY PARKING MANEUVERS. CORRECTION: A NEW RETURN POWER STEERING HOSE KIT HAS BEEN DEVELOPED TO CORRECT STEERING SHUDDER. PART NUMBER 7841445 IS FOR THE 2.5L L-4 ENGINE AND PART NUMBER 7841446 IS FOR THE 2.8L V-6 ENGINE. PROCEDURE: 1.DISCONNECT RETURN PIPE AT STEERING GEAR. 2.DISCONNECT RETURN HOSE AT POWER STEERING PUMP RETURN PIPE AND DISCARD PIPE AND HOSE. 3.INSTALL NEW RETURN HOSE AT STEERING GEAR AND TORQUE FITTING TO 27 N.M(20 FT. LBS.). 4.INSTALL NEW HOSE ON POWER STEERING PUMP PIPE AS SHOWN IN FIG. 1 AND 2. NOTE THE ILLUSTRATIONS VIEW A TO ASSURE PROPER DIMENSION. ON V6 ENGINE INSTALL A PLASTIC TIE STRAP AS SHOWN IN FIG. 2. 5.FILL AND BLEED SYSTEM. REFER TO THE BLEEDING POWER STEERING SYSTEM IN THE 1981 OMEGA SERVICE MANUAL SECTION 3B2. PARTS INFORMATION: THE KITS ARE AVAILABLE FROM GM PARTS (GMWDD). PART NUMBER 7841445 USAGE 2.5 L L-4 ENGINE PART NUMBER 7841446 USAGE 2.8L V-6 ENGINE

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.