RECOMMENDED RTV SEALANTS P/N'S AND APPLICATIONS. Chevrolet Citation 1980

For 1990-2009 cars

# RECOMMENDED RTV SEALANTS P/N'S AND APPLICATIONS

#### Model and Year: ALL ENGINES IN CHEVROLET VEHICLES

#### TO: ALL CHEVROLET DEALERS

The following chart lists the current engineering recommended sealants to be used.

These sealants, when applied properly, offer better sealing than previously recommended sealers.

Therefore, when ordering RTV sealants through WDDGM, use those sealers as listed below:

#### GENERAL MOTORS SERVICE APPROVED RTV SILICONE SEALANTS

Part Name Color Part No. Size Application --------- ----- --------- ---- ----------- GMS(Type B) Black 01052914 300 ML Caulker Chevrolet & Buick 01052917 3 Oz Tube Manufactured Engines

GMS(Type A) Clear 01052915 300 ML Caulker Pontiac, Oldsmobile and Cadillac Manufactured Engines (Except Cadillac Plastic Rocker Covers)

GE Silimate Black 01052751 3 Oz Tube Cadillac Plastic Rocker Covers Only

GMS Red 01052366 3 Oz Tube Rear Axle Usage Only

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.