CODE 34 DIAGNOSTIC PROCEDURE POSSIBLE PROM REPLACEMENT. Chevrolet Citation 1982

For 1990-2009 cars

# CODE 34 DIAGNOSTIC PROCEDURE POSSIBLE PROM REPLACEMENT

#### Model and Year 1982 CAVALIER, CHEVETTE CITATION AND CAMARO

This information applies to Federal and California 1982 Cavaliers and California only 1982 Chevettes with manual transmissions and 1982 Citation and Camaro with manual transmission and 2.8L V6 engines (engine Code X in Citation and Code 1 in Camaro).

When diagnosing a vehicle exhibiting a Code 34 (map sensor), the diagnostic charts in Section 6E of the service manual should be followed. If the diagnostic chart indicates the map sensor is functioning properly, a new PROM should be installed as shown on the attached chart. This PROM has been calibrated to prevent a Code 34 from being set when the map sensor is functioning properly.

#### NOTICE: The ECM part number of the 1982 Cavalier will have to be known in order to select the proper replacement PROM. This number is located in the upper right hand corner of the ECM identification label. This label is located on the ECM, next to the PROM access window.

#### SERVICE PROM APPLICATION CHART

Service PROM Model ECM Part Number* Package ----- ------------------- ------- *See Notes A and B at End of Chart

#### 1982 Camaro (1FAO00)

2.8L V6, Federal Emission System 16025371 (A) 1225916

1982 Chevette (1TA00)

1.6L L4, California Emission System 16017171 (A) 1225566

#### 1982 Citation (1XA00)

2.8L V6, Federal Emission System 16017191 (A) 1225767

#### 1982 Cavalier

All models with 4:10 Axle 16026231 (A) 1225752

Station Wagon (1JD35)

- With A/C 16020521 (A) 1225754 16023801 (B) 1226718 16018211 (B) 1226718

- Without A/C 16020531 (A) 1225755 16023811 (B) 1226719 16018251 (B) 1226719

Two Door Notchback (1JD27)

With A/C 16020381 (A) 1225757 16023761 (B) 1226716 16018161 (B) 1226716

Without A/C

Federal w/Manual Steering 16020541 (A) 1225756 Federal w/Power Steering 16020391 (A) 1225589 All California 16020391 (A) 1225589

*See Notes A and B at End of Chart

Two Door Hatchback (1JD77)

- With A/C 16020381 (A) 1225757 16023761 (B) 1226716 16018161 (B) 1226716

- Without A/C

With Power Steering 16020391 (A) 1225589 16023771 (B) 1226717 16018201 (B) 1226717

With Manual Steering 16023821 (B) 1226720 16018101 (B) 1226720

Four Door Notchback (1JD69)

- With A/C 16020381 (A) 1225757 16023761 (B) 1226716 (16018161)(B) 1226716

- Without A/C

With Power Steering 16020391 (A) 1225589 16023771 (B) 1226717 16018201 (B) 1226717 With Manual Steering 16023821 (B) 1226720 16018101 (B) 1226720

NOTE A: This ECM may have been replaced by service ECM, P/N 16019710 (1225500).

NOTE B: This ECM may have been replaced by service ECM, P/N 16018000 (1225330).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.