Approximate Fluid Capacities. Chevrolet Evaluator 1985

For 1990-2009 cars

#### Fluid Capacities

Application | Specification
--- | ---
Metric | English
Important: All capacities are approximate. When adding, be sure to fill to the appropriate level, as recommended in this manual.
Air Conditioning Refrigerant R134a Use Refrigerant Oil, R134a Systems | 0.6 kg | 1.3 lb
Automatic Transaxle Complete Overhaul | 9.0 L | 9.5 qts
Engine Cooling

- 2.2L Engine

6.3 L

6.7 qts

- 3.5L Engine

9.6 L

10 qts

Engine Oil with Filter

- 2.2L Engine

4.7 L

5.0 qts

- 3.5L Engine

3.8 L

4.0 qts

Fuel Tank | 62.5 L | 16.5 gals
Power Steering System | 0.70 L | 1.5 pts
Wheel Nut Torque | 140 N·m | 100 lb ft

#### Engine Specifications

Engine | VIN Code | Transaxle | Spark Plug Gap
--- | --- | --- | ---
2.2L L4 | F | Automatic | 1.0 mm (0.040 in)
3.5L LX9 | 8 | Automatic | 1.5 mm (0.060 in)