Scan Tool Data List. Chevrolet Evaluator 1985

For 1990-2009 cars

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition On, Engine Off, All Doors Closed
Accessory Relay Command | Outputs | On/Off | Off
Auto Door Locks Mode | Data | Enabled/Disabled | Enabled
Auto Door Unlock Method | Data | Key/Park | Park
Auto Door Unlock Mode | Data | None/Driver/All/Invalid | Driver
Battery Voltage | Data | Volts | 12.8 V
Door Ajar Switch | Inputs | Door Closed/Door Ajar | Door Closed
Door Cylinder Switch | Inputs | Idle/Lock/Unlock | Idle
Door Cylinder Switch | Outputs | Volts | Volts
Door Lock Switch | Inputs | Idle/Lock/Unlock | Idle
Door Lock Switch | Outputs | Volts | Volts
Driver Door Ajar Switch | Inputs | Door Closed/Door Ajar | Door Closed
Driver Door Lock Actuator Command | Outputs | Idle/Lock/Unlock/Invalid | Idle
Key Lock/Unlock Enable | Data | Enabled/Disabled | Enabled
Passenger Doors Lock Actuator Command | Outputs | Idle/Lock/Unlock/Invalid | Idle
Rear Defog Relay Command | Outputs | ON/OFF | OFF
Rear Defog Switch | Inputs | ON/OFF | OFF