Frame - Front. Chevrolet Evaluator 1985

For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Notice , in Cautions and Notices. Lifting and Jacking Caution. Refer to (Link Disabled-For Test) in Cautions and Notices. Battery Disconnect Caution in Cautions and Notices.
1 | Bolt, Side Rail Reinforcement (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten: to 100 N·m (74 lb ft).
2 | Bolt, Front Suspension Frame (Qty: 4) Tighten: to First Pass 100 N·m (74 lb ft). Final Pass + 90°.
3 | Reinforcement, Left Side Rail
4 | Reinforcement, Right Side Rail
5 | Retainer, Frame Insulator (Qty: 2)

6

Frame, Drivetrain and Front Suspension

- Tip: Tie a rope around the radiator/condenser tabs and the upper tie bar to support the radiator/condenser.

#### Tools Required

• | J 28467-B Universal Engine Support Fixture

• | J 36462 Engine Support Adapter Leg

7 | Bolt, Condenser Radiator Fan Module Support Bracket (Qty: 2) Tighten: to 60 N·m (44 lb ft).
8 | Bracket, Left Condenser Radiator Fan Module Support
9 | Bracket, Right Condenser Radiator Fan Module Support
10 | Insulator, Frame Upper (Qty: 4)
11 | Insulator, Frame Rear (Qty: 2)
12 | Insulator, Frame Front (Qty: 2)