FRONT BRAKE PAD WEAR ADJUST BRAKE PEDEL PUSH ROD. Chevrolet Nova 1988

For 1990-2009 cars

# FRONT BRAKE PAD WEAR ADJUST BRAKE PEDEL PUSH ROD

#### Model and Year: 1985-88 NOVA

Some of the subject vehicles may experience above normal front brake pad wear.

This condition may result from improper adjustment of the brake pedal push rod.

Using procedures described in the service manual, check brake pedal height and pedal freeplay and adjust brake pedal push rod length as appropriate.

Labor Operation Number: T1386

Labor Time : .4 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.