For 1990-2009 cars

Most stationary windows, specifically windshields, are retained to the body with urethane adhesive which adheres the window to the body. This increases structural integrity. The reinstallation of windows with urethane adhesive requires complete replacement of the urethane adhesive bead:

The extended method (also known as long method, full strip or full cut) is the only recommended procedure for General Motor Vehicle.