For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the HVAC module assembly. Refer to HVAC Module Assembly Replacement .
2. Remove the heater core cover. Refer to Heater Core Cover Replacement .
3. Remove the air inlet assembly. Refer to Air Inlet Assembly Replacement .
4. Note routing of electrical wiring to ensure proper installation.
5. Disconnect electrical connectors.

1 | Rear Air Outlet Duct Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Rear Air Outlet Duct
3 | Evaporator Case Drain Tube Seal
4 | Evaporator Case Assembly Screw (Qty: 10) Tighten 1.5 N·m (13 lb in)
5 | Air Distributor
6 | Evaporator Case - Lower
7 | Evaporator Case - Upper
8 | Evaporator Core
9 | Blower Motor Resistor Screw (Qty: 2) Tighten 1.5 N·m (13 lb in)
10 | Blower Motor Screw (Qty: 2) Tighten 1.5 N·m (13 lb in)
11 | Blower Motor Assembly
12 | Air Inlet Housing Baffle