For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the radiator air upper baffle and deflector. Refer to Radiator Air Upper Baffle and Deflector Replacement.
2. Remove the charge air cooler inlet pipe. Refer to Charge Air Cooler Inlet Pipe Replacement.
3. Remove the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement.
4. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
5. Remove the air cleaner duct. Refer to Air Cleaner Outlet Duct Replacement.

1 | Radiator Assembly Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Cooling Fan and Motor Shroud Assembly

#### Procedure

Disconnect the cooling fan motor electrical connector.