For 1990-2009 cars

#### Tools Required

J 42067 Rear Main Seal Installer

1. Remove excess sealer from seal recess.
2. Lubricate the outside diameter of the new crankshaft seal with clean engine oil.
3. Using the J 42067 , press the new crankshaft seal into the housing. The J 42067 also establishes the depth of the seal in the crankshaft seal bore. The seal should be flush to 0.5 mm (0.0197 in) deep.