For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Brake Dust Caution in the Preface section.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation .
3. Remove the rear disc brake pads. Refer to Rear Disc Brake Pads Replacement .

1 | Brake Caliper Bracket Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 115 N·m (85 lb ft)
2 | Brake Caliper Bracket

#### Procedure

1. If reinstalling the caliper bracket, thoroughly clean the brake pad mating surfaces of the bracket of any debris and corrosion.
2. Before reinstalling the caliper bracket, inspect the bracket to ensure it is not bent, cracked or damaged. If the bracket exhibits any of these conditions, the bracket requires replacement.