For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the fuse labeled HVAC CTRL (BATT).
2. Remove the knee bolster. Refer to Knee Bolster Replacement .

1 | Air Temperature Actuator Screw (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Air Temperature Actuator - Right

#### Procedure

• | Disconnect the right air temperature electrical connector.

• | Recalibrate the Actuator. Refer to Actuator Recalibration