For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Inflatable Restraint Front End Discriminating Sensor Stud (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Loosen the studs and slide the module up and out of the keyhole slots.

Tighten
8 N·m (71 lb in)

2 | Inflatable Restraint Front End Discriminating Sensor Assembly Warning: Do not strike or jolt the inflatable restraint front end sensor. Before applying power to the front end sensor make sure that it is securely fastened. Failure to observe the correct installation procedure could cause SIR deployment, personal injury, or unnecessary SIR system repairs.

Warning: Refer to SIR Warning in the Preface section.