For 1990-2009 cars

## Evaporator Tube Replacement First Design

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the air inlet grille. Refer to Air Inlet Grille Panel Replacement.

1 | A/C Condenser Tube Assembly Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

3 | A/C Compressor and Condenser Hose Assembly Nut Tighten 9 N·m (80 lb in)
4 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

5 | A/C Evaporator Hose Assembly Clip Nut (Qty: 2) Tighten 9 N·m (80 lb in)
6 | A/C Evaporator Hose Assembly Bolt (Qty: 2) Tighten 16 N·m (12 lb ft)
7 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

8 | A/C Evaporator Hose Assembly