For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Driver or Passenger Seat Replacement.
2. Remove the front seat cushion cover and pad. Refer to Seat Cushion Trim Cover and Pad Replacement.

1 | Seat Cushion Frame Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Seat Cushion Frame Assembly

#### Procedure

1. Disconnect any wiring connectors, if equipped.
2. If working on the passenger seat, re-zero the inflatable restraint passenger presence system whenever the seat cushion or any component of the passenger presence system is removed. Refer to Control Module References.