For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Driver and Passenger Seat Replacement .
2. Remove the front seat cushion cover and pad. Refer to Seat Cushion Trim Cover and Pad Replacement .

1 | Seat Cushion Frame Bolt (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Seat Cushion Frame Assembly

#### Procedure

1. Disconnect any wiring connectors, if equipped.
2. If working on the passenger seat, re-zero the inflatable restraint passenger presence system whenever the seat cushion or any component of the passenger presence system is removed. Refer to Control Module References .