For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the intake manifold cover. Refer to Intake Manifold Cover Replacement.
2. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
3. Remove the power steering pump pulley. Refer to Power Steering Pump Pulley Replacement.

1 | Power Steering Fluid Reservoir Outlet Hose Clamp

#### Procedure

Remove as much power steering fluid as possible from the remote power steering fluid reservoir.

2 | Power Steering Fluid Reservoir Outlet Hose
3 | Power Steering Gear Inlet Hose Fitting Caution: Refer to Fastener Caution in the Preface section. Tighten 27 N·m (20 lb ft)
4 | Power Steering Pump Bolt (Qty: 3) Tighten 22 N·m (16 lb ft)
5 | Power Steering Pump

#### Procedure

1. Remove the power steering pump from the top of the vehicle.
2. Fill and bleed the power steering system. Refer to Power Steering System Bleeding.