For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the charge air cooler. Refer to Charge Air Cooler Replacement .
3. Remove the lower radiator air baffle. Refer to Radiator Air Lower Baffle and Deflector Replacement .
4. Remove the upper radiator air baffle. Refer to Radiator Air Upper Baffle and Deflector Replacement .

1 | Receiver Dehydrator Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Receiver Dehydrator Screw Tighten 1.5 N·m (13 lb in)
3 | Receiver Dehydrator O-Ring

#### Procedure

Remove and discard the O-rings.

4 | Receiver Dehydrator Assembly