For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement .
3. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement .
4. Remove the generator. Refer to Generator Replacement .
5. Remove the drive belt. Refer to Drive Belt Replacement .

1 | A/C Compressor and Condenser Hose Assembly Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Sealing Washer

#### Procedure

Remove and discard the sealing washer. Refer to Sealing Washer Replacement .

3 | A/C Compressor Bolt (Qty: 3)

#### Procedure

Tighten the bolts in sequence.

Tighten
22 N·m (16 lb ft)

4 | A/C Compressor Assembly