For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Door Water Deflector Replacement.
3. Remove the outside door handle. Refer to Door Outside Handle Replacement.

1 | Lock Cylinder Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Side Door Outside Handle Lock Cylinder