For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel (I/P) compartment. Refer to Instrument Panel Compartment Replacement.

1 | Blower Motor Resistor Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the blower motor resistor electrical connector.

Tighten
1.5 N·m (13 lb in)

2 | Blower Motor Resistor
3 | Blower Motor Screw (Qty: 3) Tighten 1.5 N·m (13 lb in)
4 | Blower Motor Assembly