For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
2. Disconnect the ignition coil electrical connector(s).
3. Remove the ignition coil bolt(s).
4. Remove the ignition coil(s).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the ignition coil(s).
2. Install the ignition coil bolt(s) and tighten to 10 N·m (89 lb in).
3. Connect the ignition coil electrical connector(s).
4. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.