For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster. Refer to Knee Bolster Replacement .
2. Disconnect the accelerator pedal position (APP) sensor electrical connector.
3. Remove the APP sensor nuts.
4. Remove the APP sensor from the vehicle.

### Installation Procedure

1. Install the APP sensor to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the APP sensor nuts .

Tighten
Tighten the nuts to 10 N·m (89 lb in).

3. Connect the APP sensor electrical connector.
4. Confirm that the APP sensor connector locking clip is fully secured.
5. Verify the operation of the accelerator pedal.
6. Install the knee bolster. Refer to Knee Bolster Replacement .