For 1990-2009 cars

#### Special Tools

• | J 39570 Chassis Ear

• | J 41416 Ultrasonic Leak Detector

| Important: Squeaks and rattles are caused by improperly controlled relative motion between vehicle components. There are 4 ways to prevent squeaks and rattles. To aid in diagnosing, use J 39570 or J 41416 .

• | Attach the component that squeaks or rattles securely.

• | Separate the components that squeak or rattle to prevent contact.

• | Insulate the components that squeak or rattle.

• | Insulate low uniform friction surfaces to eliminate stickslip motion.