For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat. Refer to Driver and Passenger Seat Replacement .

1 | Seat Back Recliner Release Trigger

#### Procedure

Pull to remove the plastic trigger cap.

2 | Seat Back Recliner Release Escutcheon

#### Procedure

Unzip the seat back cushion cover and press the tabs inward on the escutcheon to release.

3 | Seat Back Cushion Cover

#### Procedure

1. Completely unzip the seat back cushion cover.
2. Disconnect the J-channel at the bottom of the seat back cushion cover.
3. Pull the seat back cushion cover and pad off the seat frame as an assembly.

4 | Seat Back Cushion Cover Pad Tip The pad is secured to the cushion cover with hook and loop fasteners. Pull apart to remove.