For 1990-2009 cars

#### Special Tools

J 43650 Balance Shaft Bushing Remover/Installer

For equivalent regional tools, refer to Special Tools

Note: Service the balance shafts as an assembly. Do not disassemble or assemble the balance shafts.

1. Install the balance shaft bushing using the J 43650 installer .
2. Seat the balance shaft bushing into the bore using the J 43650 installer and a wrench.
3. When the J 43650 installer is fully seated in the engine block, remove it with a wrench.

Note: If the balance shafts are not properly timed to the engine, the engine may vibrate or make noise.

4. Install the balance shaft assemblies to the engine using the following steps:

4.1. | Place the number 1 piston at top dead center (TDC).

4.2. | Lubricate the balance shaft lobes with engine oil.

4.3. | Install the balance shafts into their bores.

Caution: Refer to Fastener Caution in the Preface section.

5. Install the balance shaft retaining bolts and tighten to 10 N·m (89 lb in).