For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Driver or Passenger Seat Replacement.
2. Remove the seat cushion cover. Refer to Seat Cushion Trim Cover and Pad Replacement.

1 | Inflatable Restraint Front Passenger Presence System Assembly Warning: Replace the passenger presence system as a complete assembly to prevent possible injury to the occupant. All the components in the service kit are assembled and calibrated as a unit. Using only some of the components in the service kit will cause the passenger presence system to operate improperly.

Warning: To avoid personal injury, perform a preload test on the passenger presence system whenever you remove or replace the seat cushion trim. Failure to do so may cause the system to malfunction.

#### Procedure

1. Re-zero the inflatable restraint passenger presence system whenever the seat cushion or any component of the passenger presence system is removed. Refer to Control Module References.
2. Program the inflatable restraint passenger presence system after replacement. Refer to Control Module References.