For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Door Water Deflector Replacement.
3. Remove the front side door window. Refer to Front Side Door Window Replacement.

1 | Window Regulator Nut Access Plug Tip Use a plastic flat-bladed tool to remove the plug from the bottom of the door.
2 | Front Side Door Window Regulator Nut (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
3 | Front Door Window Regulator Bolt (Qty: 3) Tighten 10 N·m (89 lb in)
4 | Front Door Power Window Regulator Tip Disconnect the electrical connector from the regulator.