For 1990-2009 cars

### Removal Procedure

1. Remove the right engine mount. Refer to Engine Mount Replacement - Right Side .
2. Remove the engine mount bracket bolts and bracket.

### Installation Procedure

1. Position the right engine mount bracket to the engine block.
2. Install the engine mount bracket bolts until snug.

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the right engine mount bracket bolts in the following sequence.

Tighten
Tighten the bolts to 55 N·m (41 lb ft).

3.1. | Lower rear

3.2. | Upper front

3.3. | Lower front

3.4. | Upper rear

4. Install the right engine mount. Refer to Engine Mount Replacement - Right Side .