For 1990-2009 cars

#### Tools Required

• | J 8092 Universal Driver Handle

• | J 44766 Seal Installer

1. Assemble J 8092 onto J 44766 .

Notice: Install the seal onto the installation tool before installing into the case to prevent damage to the seal.

2. Install the seal (229) onto J 44766 .

Important: Align the torque converter seal with the bolt holes.

3. Install the NEW seal (229) into the housing.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the NEW seal bolts (228).

Tighten
Tighten the seal bolts to 3.6 N·m (31.86 lb in).

5. Install the NEW input shaft seal (430).