For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the folding top and stowage compartment lid.
2. Remove the upper garnish molding. Refer to Windshield Upper Garnish Molding Replacement .

1 | Receiver Pin Front Locating Folding Top Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tip Mark the location of the receiver before removing. Tighten
25 N·m (18 lb ft)

2 | Pin Front Locating Folding Top Receiver